Inputs:

1, 2, 3, 4, 5, 6, 7, 8, 9, 11

Outputs:

12 (Combinatorial, No output feedback, Active low)
13 (Combinatorial, No output feedback, Active low)
14 (Combinatorial, No output feedback, Active low)
15 (Combinatorial, No output feedback, Active low)
16 (Combinatorial, No output feedback, Active low)
17 (Combinatorial, No output feedback, Active low)
18 (Combinatorial, No output feedback, Active low)
19 (Combinatorial, No output feedback, Active low)

Equations:

/o12 = /i1 & i7 +
       i8 +
       i9 & i11 +
       i2 +
       i1 & i3 +
       i5 +
       i4 & /i11 +
       i6
o12.oe = vcc

/o13 = /i8 +
       /i11 +
       /i9 +
       /i3 & /i6 +
       /i1 & /i7 +
       /i2 +
       /i4 +
       /i5
o13.oe = vcc

/o14 = /i3 & /i9 +
       /i6 +
       /i2 +
       i4 +
       /i8 & i11 +
       i7 +
       i5 & /i11 +
       /i1
o14.oe = vcc

/o15 = i4 +
       i1 & /i3 +
       i2 & i9 +
       i5 +
       i1 & i7 +
       /i3 +
       /i8 +
       /i1
o15.oe = vcc

/o16 = i6 +
       /i2 & /i9 +
       i3 & i11 +
       /i8 +
       i6 & i8 +
       /i1 +
       /i5 & i7 & i8 +
       /i7 & /i8
o16.oe = vcc

/o17 = i3 & i4 +
       /i5 +
       /i9 +
       /i1 & /i11 +
       i7 +
       i2 & i9 +
       i6 & i9 +
       /i8
o17.oe = vcc

/o18 = /i9 +
       i3 & i5 & i9 +
       /i7 +
       /i11 +
       /i1 +
       /i3 +
       /i5 +
       i1 & i7 & i11
o18.oe = vcc

/o19 = /i3 & /i5 & /i7 +
       i2 +
       i8 +
       i3 & i11 +
       i1 +
       i4 +
       i6 +
       /i1 & /i9
o19.oe = vcc

