Inputs:

2, 3, 4, 5, 6, 7, 8, 9, 12, 13, 14, 15, 16, 17, 18, 19

Outputs:

12 (Registered, Output feedback registered, Active low)
13 (Registered, Output feedback registered, Active low)
14 (Registered, Output feedback registered, Active low)
15 (Registered, Output feedback registered, Active low)
16 (Registered, Output feedback registered, Active low)
17 (Registered, Output feedback registered, Active low)
18 (Registered, Output feedback registered, Active low)
19 (Registered, Output feedback registered, Active low)

Equations:

/rf12 := /i2 & /i3 +
         i4 & rf13 +
         i3 +
         /i6 +
         i8 +
         /i9 +
         i7 & /rf13 +
         i5
rf12.oe = OE

/rf13 := /rf14 +
         /i9 +
         i8 +
         /i7 +
         /i6 & rf14 +
         i5 +
         i4 +
         /i3
rf13.oe = OE

/rf14 := /rf15 +
         /i8 +
         i8 +
         /i2 & /rf15 +
         /i2 +
         i2 & /i8 & rf15 +
         /i4 +
         i3
rf14.oe = OE

/rf15 := i3 & i6 & i7 +
         i6 & rf16 +
         i3 & /rf16 +
         i7 +
         /i4 +
         i6 & i7 +
         i4 & i7 +
         /i2 & /i7
rf15.oe = OE

/rf16 := /i3 & /rf17 +
         /i4 +
         /i3 +
         /i3 & i4 +
         /i7 & rf17 +
         /i7 +
         i4 +
         i2 & i3
rf16.oe = OE

/rf17 := i2 & i5 & i6 & /i7 +
         i2 & /rf18 +
         i5 +
         i6 +
         /i7 & rf18 +
         i2 & /i7 +
         i5 & i6 +
         /i3
rf17.oe = OE

/rf18 := /i2 & i5 & i6 & /i7 +
         i3 & i6 & i7 +
         i3 & rf19 +
         /i2 & /i7 +
         /i3 & /rf19 +
         i5 & i6 & /i7 +
         i7 +
         /i4
rf18.oe = OE

/rf19 := i5 & i6 & /i7 +
         i3 & i6 & i7 +
         i5 & rf12 +
         i6 +
         i7 +
         /i4 & /rf12 +
         /i7 +
         i2
rf19.oe = OE

