Inputs:

1, 2, 3, 4, 5, 6, 7, 8, 9, 11

Outputs:

12 (Combinatorial, No output feedback, Active high)
13 (Combinatorial, No output feedback, Active high)
14 (Combinatorial, No output feedback, Active high)
15 (Combinatorial, No output feedback, Active high)
16 (Combinatorial, No output feedback, Active high)
17 (Combinatorial, No output feedback, Active high)
18 (Combinatorial, No output feedback, Active high)
19 (Combinatorial, No output feedback, Active high)

Equations:

o12 = i2 +
      i1 & i3 +
      i4 & /i11 +
      i5 +
      i6 +
      /i1 & i7 +
      i8 +
      i9 & i11
o12.oe = vcc

o13 = /i2 +
      /i4 +
      /i3 & /i6 +
      /i8 +
      /i11 +
      /i9 +
      /i1 & /i7 +
      /i5
o13.oe = vcc

o14 = i4 +
      /i8 & i11 +
      /i6 +
      /i2 +
      i5 & /i11 +
      i7 +
      /i3 & /i9 +
      /i1
o14.oe = vcc

o15 = i5 +
      /i1 +
      i1 & i7 +
      /i3 +
      i1 & /i3 +
      i2 & i9 +
      /i8 +
      i4
o15.oe = vcc

o16 = i6 +
      i3 & i11 +
      i6 & i8 +
      /i1 +
      /i8 +
      /i7 & /i8 +
      /i2 & /i9 +
      /i5 & i7 & i8
o16.oe = vcc

o17 = i7 +
      i2 & i9 +
      i3 & i4 +
      /i5 +
      /i9 +
      /i8 +
      /i1 & /i11 +
      i6 & i9
o17.oe = vcc

o18 = /i1 +
      /i3 +
      /i5 +
      /i7 +
      /i9 +
      /i11 +
      i1 & i7 & i11 +
      i3 & i5 & i9
o18.oe = vcc

o19 = i3 & i11 +
      i1 +
      /i1 & /i9 +
      /i3 & /i5 & /i7 +
      i2 +
      i4 +
      i6 +
      i8
o19.oe = vcc

