Inputs:

1, 2, 3, 4, 5, 6, 7, 8, 9, 11

Outputs:

12 (Combinatorial, No output feedback, Active high)
13 (Combinatorial, No output feedback, Active high)
14 (Combinatorial, No output feedback, Active low)
15 (Combinatorial, No output feedback, Active low)
16 (Combinatorial, No output feedback, Active high)
17 (Combinatorial, No output feedback, Active low)
18 (Combinatorial, No output feedback, Active low)
19 (Combinatorial, No output feedback, Active low)

Equations:

o12 = i9 & i11 +
      /i1 & i2 & i3 & i4 & i5 & i6 & /i7 & i8
o12.oe = vcc

o13 = i9 & /i11 +
      i1 & /i2 & i3 & i4 & i5 & /i6 & i7 & i8
o13.oe = vcc

/o14 = /i9 & /i11 +
       i1 & i2 & /i3 & i4 & /i5 & i6 & i7 & i8
o14.oe = vcc

/o15 = /i9 & i11 +
       i1 & i2 & i3 & /i4 & i5 & i6 & /i7 & i8
o15.oe = vcc

o16 = i9 & /i11 +
      i1 & i2 & i3 & i4 & i5 & /i6 & i7 & /i8
o16.oe = vcc

/o17 = i9 & i11 +
       /i1 & /i2 & i3 & i4 & i5 & i6 & /i7 & /i8
o17.oe = vcc

/o18 = /i9 & /i11 +
       i1 & i2 & i3 & /i4 & /i5 & i6 & i7 & i8
o18.oe = vcc

/o19 = /i9 & i11 +
       i1 & /i2 & i3 & /i4 & i5 & /i6 & i7 & /i8
o19.oe = vcc

