Inputs:

1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 13, 14, 23

Outputs:

15 (Combinatorial, No output feedback, Active low)
16 (Combinatorial, No output feedback, Active low)
17 (Combinatorial, No output feedback, Active low)
18 (Combinatorial, No output feedback, Active low)
19 (Combinatorial, No output feedback, Active low)
20 (Combinatorial, No output feedback, Active low)
21 (Combinatorial, No output feedback, Active low)
22 (Combinatorial, No output feedback, Active low)

Equations:

/o15 = /i1 & /i2 +
       /i3 +
       /i4 +
       /i5 & /i6
o15.oe = vcc

/o16 = /i7 +
       /i8
o16.oe = vcc

/o17 = /i9 & /i10 +
       /i13
o17.oe = vcc

/o18 = i1 & i2 & i3 +
       i4 & i5 & i6 & /i14
o18.oe = vcc

/o19 = i7 +
       i8
o19.oe = vcc

/o20 = i9 & i10 & i14 +
       i13
o20.oe = vcc

/o21 = /i2 & i5 & i6 & /i7 +
       i3 & i6 & i7 & i13 & i23
o21.oe = vcc

/o22 = i5 & i6 +
       /i7 & i11 +
       /i23 +
       /i1 & i3 & i6 & i7 & i10
o22.oe = vcc

