Inputs:

1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 13

Outputs:

14 (Combinatorial, No output feedback, Active high)
15 (Combinatorial, No output feedback, Active high)
16 (Combinatorial, No output feedback, Active high)
17 (Combinatorial, No output feedback, Active high)
18 (Combinatorial, No output feedback, Active high)
19 (Combinatorial, No output feedback, Active high)
20 (Combinatorial, No output feedback, Active high)
21 (Combinatorial, No output feedback, Active high)
22 (Combinatorial, No output feedback, Active high)
23 (Combinatorial, No output feedback, Active high)

Equations:

o14 = /i1 & /i2 & /i3 +
      /i4 & /i5 & /i6
o14.oe = vcc

o15 = /i7 +
      /i8
o15.oe = vcc

o16 = /i9 & /i10 +
      /i13
o16.oe = vcc

o17 = i1 & i2 & i3 +
      i4 & i5 & i6
o17.oe = vcc

o18 = i7 +
      i8
o18.oe = vcc

o19 = i9 & i10 +
      i13
o19.oe = vcc

o20 = /i2 & i5 & i6 & /i7 +
      i3 & i6 & i7 & i13
o20.oe = vcc

o21 = i5 & i6 & /i7 & i11 +
      /i1 & i3 & i6 & i7 & i10
o21.oe = vcc

o22 = i4 & i13 +
      i9 & /i10 & /i11
o22.oe = vcc

o23 = /i4 & i10 & i11 +
      i1 & /i13
o23.oe = vcc

