Inputs:

1, 2, 3, 4, 5, 6, 7, 8, 9, 11

Outputs:

12 (Combinatorial, No output feedback, Active low)
13 (Combinatorial, No output feedback, Active low)
14 (Combinatorial, No output feedback, Active low)
15 (Combinatorial, No output feedback, Active low)
16 (Combinatorial, No output feedback, Active low)
17 (Combinatorial, No output feedback, Active low)
18 (Combinatorial, No output feedback, Active low)
19 (Combinatorial, No output feedback, Active low)

Equations:

/o12 = /i1 & i2 & i3 & i4 & i5 & i6 & i7 & i8 +
       i9 & i11
o12.oe = vcc

/o13 = i1 & /i2 & i3 & i4 & i5 & i6 & i7 & i8 +
       /i9 & i11
o13.oe = vcc

/o14 = i1 & i2 & /i3 & i4 & i5 & i6 & i7 & i8 +
       i9 & /i11
o14.oe = vcc

/o15 = i1 & i2 & i3 & /i4 & i5 & i6 & i7 & i8 +
       /i9 & /i11
o15.oe = vcc

/o16 = i1 & i2 & i3 & i4 & /i5 & i6 & i7 & i8 +
       /i9 & /i11
o16.oe = vcc

/o17 = i1 & i2 & i3 & i4 & i5 & /i6 & i7 & i8 +
       i9 & /i11
o17.oe = vcc

/o18 = i1 & i2 & i3 & i4 & i5 & i6 & /i7 & i8 +
       i11
o18.oe = vcc

/o19 = i1 & i2 & i3 & i4 & i5 & i6 & i7 & /i8 +
       /i9
o19.oe = vcc

