Inputs:

1, 2, 3, 4, 5, 6, 7, 8, 9, 11, 12, 13, 14, 15, 16, 17, 18, 19

Outputs:

9 (Combinatorial, Output feedback output, Active high)
11 (Combinatorial, Output feedback output, Active low)
12 (Combinatorial, Output feedback output, Active high)
13 (Combinatorial, Output feedback output, Active low)
14 (Combinatorial, Output feedback output, Active high)
15 (Combinatorial, Output feedback output, Active low)
16 (Combinatorial, Output feedback output, Active high)
17 (Combinatorial, Output feedback output, Active low)
18 (Combinatorial, Output feedback output, Active high)
19 (Combinatorial, Output feedback output, Active low)

Equations:

o9 = i1 & i2 +
     /i3 +
     o19 +
     /i4 +
     /i5 +
     i6 +
     i7 +
     /i8 & /o19
o9.oe = vcc

/o11 = /i1 +
       /i2 +
       i5 +
       /i6 +
       /i7 +
       i8 +
       i4 & o9 +
       /i3 & /o9
o11.oe = vcc

o12 = i1 +
      i2 +
      i4 +
      i5 +
      i6 +
      /i8 +
      i7 & o11 +
      i3 & /o11
o12.oe = vcc

/o13 = /i1 +
       i2 +
       /i3 +
       /i4 +
       /i6 +
       i8 +
       /i7 & o12 +
       /i5 & /o12
o13.oe = vcc

o14 = /i2 & /i3 & /i4 +
      i4 & i5 +
      i2 & /i6 +
      i3 & i7 +
      i6 & /i7 +
      i8 +
      /i2 & i3 & /i5 & i8 +
      /i1 & /i8 +
      i2 & /i7 & o13 +
      i1 & /o13
o14.oe = vcc

/o15 = /i3 & /i4 +
       i5 +
       i1 & i2 & i3 & i4 & i5 +
       /i2 & i7 +
       i3 & i8 +
       /i7 & i8 +
       i6 & i7 & /i8 +
       /i4 & o14 +
       i7 & o14 +
       i6 & i7 & /i8 & /o14
o15.oe = vcc

o16 = i3 +
      /i4 +
      i5 +
      /i6 +
      i7 +
      /i8 +
      i1 & o15 +
      /i2 & /o15
o16.oe = vcc

/o17 = /i1 +
       i2 +
       /i5 +
       /i3 & i6 +
       /i6 +
       i8 +
       /i7 & o16 +
       i4 & /o16
o17.oe = vcc

o18 = /i1 +
      /i2 +
      /i3 +
      i6 +
      i7 +
      i8 +
      /i4 & o17 +
      i5 & /o17
o18.oe = vcc

/o19 = i2 +
       i3 +
       i4 +
       /i5 +
       /i6 +
       /i7 +
       i1 & o18 +
       /i8 & /o18
o19.oe = vcc

