Inputs:

1, 2, 3, 4, 5, 6, 7, 8, 9, 11, 12, 13, 14, 15, 16, 17, 18, 19

Outputs:

12 (Combinatorial, Output feedback output, Active high)
13 (Combinatorial, Output feedback output, Active high)
14 (Combinatorial, Output feedback output, Active high)
15 (Combinatorial, Output feedback output, Active high)
16 (Combinatorial, Output feedback output, Active high)
17 (Combinatorial, Output feedback output, Active high)
18 (Combinatorial, Output feedback output, Active high)
19 (Combinatorial, Output feedback output, Active high)

Equations:

o12 = /i1 & i2 & i3 & i4 & i5 & i6 & i7 & i8 +
      i9 & i11
o12.oe = vcc

o13 = i1 & /i2 & i3 & i4 & i5 & i6 & i7 & i8 +
      /i9 & i11
o13.oe = vcc

o14 = i1 & i2 & /i3 & i4 & i5 & i6 & i7 & i8 +
      i9 & /i11
o14.oe = vcc

o15 = i1 & i2 & i3 & /i4 & i5 & i6 & i7 & i8 +
      /i9 & /i11
o15.oe = vcc

o16 = i1 & i2 & i3 & i4 & /i5 & i6 & i7 & i8 +
      /i9 & /i11
o16.oe = vcc

o17 = i1 & i2 & i3 & i4 & i5 & /i6 & i7 & i8 +
      i9 & /i11
o17.oe = vcc

o18 = i1 & i2 & i3 & i4 & i5 & i6 & /i7 & i8 +
      /i9 & i11
o18.oe = vcc

o19 = i1 & i2 & i3 & i4 & i5 & i6 & i7 & /i8 +
      i11
o19.oe = vcc

